Rename the unforce_multiboxse.txt to force_multiboxse.txt and move it to the root of your usb-stick
When you enter the recovery menu then it will force to install the image M48051_maxytecmultise_v2-06_nightly_UPDATEUSB_g27772_multi.zip in the linux1 selection
