Rename the unforce_hd61.txt to force_hd61.txt and move it to the root of your usb-stick
When you enter the recovery menu then it will force to install the image M48479_ax61_v2-09_nightly_UPDATEUSB_g28007_multi.zip in the linux1 selection
